**Configuration Sheet For OPOS Mode**

**Datalogic Gryphon GD4100**

1. **Set Default**

****

**Wait to finish Beeping**

1. **Enable USB-OEM (OPOS Ode)**



**Wait to finish Beeping**

**WARNING - Only Scan the following barcode if you need to configure it back to USB keyboard mode (Default mode)**

**This mode is not compatible with Existco/Roshtek Solutions**

