**Configuration Sheet For**

**Datalogic QBT2430 PCS V2**

1. **Set Default**

****

**Wait to finish Beeping**

1. **Disable Heads and Terminators not needed**















**Wait to finish Beeping**

1. **Set USB-OEM OPOS**



1. **Re-Link (Only if needed)**

****

For RF devices, before configuring the interface it is necessary to link the handheld with the base.

To link the handheld and the base, press the trigger to wake it and place it on the base.

If the reader was previously linked to another base, you must first scan the Unlink action com­mand before re-linking to the new base.